D8224 Mullion Reader
ARCHITECTURAL AND ENGINEERING SPECIFICATION 
Section 281326 – Access Control Remote Devices
 
PART 2 – PRODUCTS

2.01	MANUFACTURER
A. Bosch Security Systems, Inc.
130 Perinton Parkway 
Fairport, New York 14450
Phone: +1(585) 223 4060
Fax: +1 (585) 223 9180
www.boschsecurity.com

B.	This product shall be manufactured by a firm whose quality system is in compliance with the I.S. /ISO 9001/EN 29001, QUALITY SYSTEM.

2.02	PROXIMITY READER DESCRIPTION
A.	The product specified is a proximity reader providing Wiegand protocol interface capability when used with Wiegand 26-bit proximity cards, tokens, and adhesive tag credentials. The unit is supplied in a weatherproof, polycarbonate enclosure designed for indoor or outdoor applications. The read range of the reader to the appropriate Wiegand credential is up to 5.5 inches (14 cm). 

2.03	PROXIMITY READER REQUIREMENTS	
A.	The product specified shall be a proximity reader that provides Wiegand protocol interface capability.

B. The reader shall have a read range of up to 5.5 inches (14 cm).

C.	The reader specified shall be compatible with ReadykeyPRO, Readykey and D9412G/D7412G Control Panels manufactured by Bosch Security Systems, Inc. 

D.	The reader shall be compatible with credentials D8236-10 Wiegand Proximity Card, D8236KF-10 Wiegand Proximity Token, and D8236TG-10 Wiegand Proximity Adhesive Tag manufactured by Bosch Security Systems, Inc.

E. Upon presentation of a compatible proximity card to the specified reader, a multicolor LED shall change from red to flashing green and a beeper will sound. The beeper and the multicolor LED shall be individually controlled either locally or from the host.

F.	The reader shall be designed for installation on a door mullion and may be directly mounted to a metal surface with minimal effect on its read range performance. The manufacturer shall supply a junction box designed for the reader that surface mounts with two screws.

G.	The reader shall be available in a charcoal gray, polycarbonate, weather-resistant enclosure suitable for indoor or outdoor applications.	 

H.	The acceptable wire length from the door controller to the reader shall be up to 500 ft. (152 m) when using 22 AWG (0.8 mm) cable.

2.04 ELECTRICAL SPECIFICATIONS:
A. Voltage (input):		5 VDC to 16 VDC
B. Current (input):		30 mA average at 5 VDC; 110 mA peak.	

2.05 MECHANICAL SPECIFICATIONS:
A. Dimensions: 6.0 in. x 1.7 in. x 1.0 in. (15 cm x 4.3 cm x 2.5 cm)
B. Weight: 3.8 oz (108 g)
C. Cabling: Minimum 22 AWG (0.8 mm) five-wire stranded with overall shield.

2.06 ENVIRONMENTAL SPECIFICATIONS:
A.		Operating Temperature:
		1)	Typical Applications: -22F to +150F (-30C to +65C)
		2)	UL 294 Applications:	-22F to +140F (-30C to +60C)
				
B.		Relative Humidity:	
		1)	Typical Applications:	0% to 95%, non-condensing
		2)	For UL Listed Applications: 0% to 85%, non-condensing

2.07 CERTIFICATIONS and APPROVALS
A. UL Standards:	UL294, Access Control System Units
B. Approvals:	FCC; CE

The product specified shall be the D8224 Mullion Reader manufactured by Bosch Security Systems, Inc.

D8224 09/5/06		Specifications subject to change without notice