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4MP OUTDOOR FIXED BOX CAMERA

[bookmark: _3dy6vkm]DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 	Video Surveillance
[bookmark: _1t3h5sf]28 21 00 	Surveillance Cameras
	28 21 13	IP Cameras 

Notes to Specifier:

[bookmark: _4d34og8]1.  Where several alternative parameters or specifications exist, or where, the specifier has the option of inserting text, such choices are presented in <bold bracketed text>.
2.  Explanatory notes and comments are presented in italicized colored text.



4MP OUTDOOR FIXED BOX CAMERA
PART  1   GENERAL
1.01 SUMMARY
A [bookmark: _2s8eyo1][bookmark: _Hlk141199083]Section includes a 4 MP outdoor fixed box camera with integrated lens, H.264 and H.265 encoding, dynamic range of 141 dB, and built-in artificial intelligence providing full situational awareness and triggers for relevant alerts.
B [bookmark: _17dp8vu]Related Requirements
1. 28 05 00 Common Work Results
2. 28 05 07.13 Power Sources for Video Surveillance
3. 28 05 07.21 PoE Power Sources for Electronic Safety and Security
4. 28 05 11 Cyber Security Requirements for Electronic Safety and Security
5. 28 05 19.13 Hybrid Digital Video Recorders
6. 28 05 19.15 Network Video Recorders
7. 28 05 33 Safety and Security Network Communications Equipment
8. 28 06 20 Schedules for Video Surveillance
9. 28 21 19 Camera Mounts
10. 28 23 00 Video Management System
11. 27 15 00 Communications Horizontal Cabling
12. 27 20 00 Data Communications 
13. 28 16 15 Access Control Interfaces to Video Surveillance
14. 28 31 31.15 Intrusion Detection Interfaces to Video Surveillance
15. 28 51 15.13 Information Interfaces to Video Surveillance Systems
C Sustainability
1. The fixed network camera shall be manufactured in compliance with ISO 9001 and ISO 14001.
2. The fixed network camera shall be compliant with the EU Directives 2011/65/EU (RoHS) and 2012/19/EU (WEEE).
3. Packaging shall be compliant with EU Directive 94/62/EC (amended by 2004/12/EC).
4. The fixed network camera shall be compliant with the EU regulation 1907/2006 (REACH).

1.02 REFERENCES
A Abbreviations
1. AI – Artificial Intelligence
2. ARP – Address Resolution Protocol
3. DHCP - Dynamic Host Configuration Protocol
4. DNS - Domain Name Server
5. DDNS – Dynamic DNS
6. DORI - Detect, Observe, Recognize, Identify
7. fps - frames per second
8. HEVC – High Efficiency Video Coding
9. HTTPS – Secure Hypertext Transfer Protocol
10. ICMP - Internet Control Message Protocol
11. IP - Internet Protocol
12. IR – InfraRed 
13. JPEG - Joint Photographic Experts Group
14. mDNS – Multicast DNS
15. MP - Megapixel
16. MJPEG - Motion JPEG
17. NTP - Network Time Protocol
18. PKI - Public Key Infrastructure
19. PoE - Power over Ethernet
20. RTCP – Real-Time Control Protocol
21. RTP - Real-Time Transport Protocol
22. RTSP - Real-Time Streaming Protocol
23. TCP - Transmission Control Protocol
24. TPM - Trusted Platform Module
25. TLS – Transport Layer Security
26. UDP - User Datagram Protocol
B Reference Standards
1. Emission
a. ANSI C63.4a
b. CISPR32 (Class A)
c. EN IEC 61000-6-4
d. EN 50121-4
e. EN 55032 (Class A), 
f. CFR 47 FCC, part 15B (class A)
g. ICES-003 Class A
h. RSS-Gen, Issue 5
i. VCCI-CISPR 32
2. Immunity
a. CISPR35
b. EN IEC 61000-6-2
c. EN 50121-4
d. EN 50130-4
e. EN 55035
3. Basic standards
a. EN 61000-4-2
b. EN 61000-4-3
c. EN 61000-4-4
d. EN 61000-4-5
e. EN 61000-4-6
f. EN 61000-4-8
4. Reliability
a. EN 50130-5 Class II-A
b. EN 60068-2-1
c. EN 60068-2-2
d. EN 60068-2-6
e. EN 60068-2-27
f. EN 60068-2-42
g. EN 60068-2-75
h. EN 60068-2-78
5. Safety
a. AS/NZS 62368.1
b. CSA C22.2 No. 62368-1
c. EN IEC 62368-1
d. GB 4943.1
e. IEC 62368-1
f. J62368-1
g. KC 62368-1
h. SASO-IEC 62368-1
i. UL 62368-1
6. Environment
a. 2011/68/EU RoHS (EN IEC 63000)
b. 1999/45/EC and 1907/2006 REACH
c. 2012/19/EU WEEE
d. 94/62/EC Packaging
e. DIN EN 62321 (PVC-free)
7. ONVIF conformance
a. IEC 626756-2-3
b. EN 60839-11-31
c. EN IEC 62676-2-31
d. EN IEC 62676-2-32 
1.03 SUBMITTALS
A Informational Submittals
1. Product Data
a. Manufacturer’s printed or electronic data sheets
b. Manufacturer’s installation and operation manuals
c. Warranty documentation
2. Shop Drawings
3. Cyber hardening guidance
B Closeout Submittals
1. Final listing of devices and settings
2. System test results
3. Statement of compliance with Manufacturer Cyber Hardening Guidelines
1.04 QUALIFICATIONS
A Installers shall be certified, trained and authorized by the Manufacturer to install, integrate, test, and commission the system.
1.05 DELIVERY, STORAGE AND HANDLING
A Deliver the camera in the manufacturer’s original, unopened, undamaged container with identification labels intact.
B Store the camera in a temperature environment protected from mechanical and environmental conditions as designated by the manufacturer.
1.06 WARRANTY AND SUPPORT
A Manufacturer shall provide a limited 5-year warranty for the product to be free of defects in material and workmanship.

END OF SECTION





PART  2 PRODUCTS
2.01 EQUIPMENT
A Manufacturer: 	Bosch Security Systems, Inc.
130 Perinton Parkway
Fairport, New York, 14450
USA
Phone: +1 800 289 0096
Fax: +1 585 223 9180
Email: security.sales@us.bosch.com
www.boschsecurity.com 

Bosch Security Systems, B.V.
P.O. Box 80002
5600 JB Eindhoven, The Netherlands
Phone: +31 40 2577 284
Fax: +31 40 2577 330
Email: emea.securitysystems@bosch.com 
www.boschsecurity.com 

Robert Bosch (SEA) Pte Ltd, Security Systems
11 Bishan Street 21
Singapore 573943
Phone: +65 6571 2600
Fax: +65 6571 2698
Email: apr.securitysystems@bosch.com
www.boschsecurity.com
B Product Model:	NBI-7803-AXT
2.02 GENERAL DESCRIPTION
A The camera shall be a 4MP fixed box type with integrated lens, starlight X, HDR X, H.264 and H.265 encoding, dynamic range of 141 dB, and built-in artificial intelligence providing full situational awareness and triggers for relevant alerts.
B The fixed box camera shall possess the following primary characteristics:
1. H.264, H.265, and MJPEG compression
2. Resolution up to 2688 x 1520 pixels 
3. Integrated 10.5-47mm lens
4. Starlight X and HDR X technology
5. Frame rate up to 60 fps
6. Suite of deep learning-based video analytics
7. Bi-directional audio
8. DORI technology to facilitate distinguishing of persons or objects 
9. Multiple data security elements including Trusted Platform Module (TPM), PKI, 4096-bit RSA encryption, and update capability for future software security functions.
10. Available posting to cloud-based services
11. Pre-configured optimized scene modes
12. Remote camera management
13. Mobile device camera setup and configuration
14. Power:	24 VAC, 12 to 26 VDC, or PoE IEEE 802.3at Type 1, Class 3
2.03 ADDITIONAL VIDEO/CAMERA SPECIFICATIONS
A Imaging Device:	
1. The fixed network camera shall offer a 1/1.8-inch CMOS image sensor.
2. The fixed network camera shall offer a maximum effective number of pixels of 2688x1520 (4.1MP).
B Lens:
1. The fixed network camera shall offer an Automatic Varifocal (AVF) lens with P-iris and a focal length of 10.5 to 47 mm.
2. The fixed network camera shall offer a lens aperture of F/1.35 to F/1.55.
3. The fixed network camera shall have a horizontal field of view of 41.6° to 9.3°.
4. The fixed network camera shall have a vertical field of view of 23.9º to 5.3º.
5. The fixed network camera shall offer automatic focus and P-iris control with manual override.
C Video Streaming:
1. The fixed network camera shall provide direct network connection using H.265, H.264 and M-JPEG compression and bandwidth throttling to efficiently manage bandwidth and storage requirements while delivering outstanding image quality.
2. The fixed network camera shall provide one M-JPEG and at least three H.264/H.265 independently configurable streams.
3. The fixed network camera shall support the following video resolutions:
a. 4.1 MP – 2688x1520 (16:9), 3.8 MP – 2592x1456 (16:9), 2.8 MP – 1920x1440 (4:3) crop, 2 MP – 1920x1080 (16:9), 1.3 MP – 1280x1024 (5:4) crop, 1.2 MP – 1280x960 (4:3) crop, 1 MP – 1280x720 (16:9), 0.5 MP – 960x544 (16:9), 0.5 MP – 800x600 (4:3) crop, VGA – 640x480 (4:3) crop, 0.2 MP – 640x360 (16:9), 0.1 MP – 480x272 (16:9)
4. The fixed network camera shall have support for both 16:9 - wide screen and 9:16 - upright aspect ratios.
5. The fixed network camera shall deliver 4MP video, at rates up to 60 images per second. 
6. The fixed network camera shall offer a High Dynamic Range of 141 dB for clear images in extreme high-contrast environments.
D [bookmark: _3rdcrjn]Additional Video Functions:
1. The fixed network camera shall support day/night modes with automatic adjustable switch points, allowing it to operate in both color and monochrome settings.
2. The fixed network camera shall include backlight compensation.
3. The fixed network camera shall offer video watermarking capabilities.
4. The fixed network camera shall provide display stamping.
5. The fixed network camera shall be capable of displaying its location information.
6. The fixed network camera shall feature electronic image stabilization to reduce the effects of camera shake.
7. The fixed network camera shall support a white balance range from 2000 K to 10,000 K.
8. The fixed network camera shall offer multiple white balance modes, including: 
a. Basic
b. Standard
c. Manual mode
d. Hold mode
e. 3 automatic modes
f. Sodium lamp
9. The fixed network camera shall allow the definition of an area within the Field of View (FOV) as an exposure priority area, enhancing the visibility of objects in that specified area.
10. The fixed network camera shall offer the ability to define up to 8 privacy masks.
11. The fixed network camera shall offer multiple user defined privacy masks patterns, including:
a. Black
b. White
c. Gray
d. Auto color
e. 16M colors
f. Mosaic
g. 10 blurred levels
12. The fixed network camera shall produce a monochrome image with a minimum scene illumination of 0.0009 lux.
13. The fixed network camera shall produce a color image with a minimum scene illumination of 0.008 lux.
14. The fixed network camera shall offer HDR (High Dynamic Range) X to enhance image quality in both bright and dark areas.
15. The fixed network camera shall offer three types of HDR X:
a. Motion optimized
b. Extreme Dynamic Range
c. Optimized Dynamic Range
16. The fixed network camera shall offer starlight X technology to deliver superior image performance in low-light environments.
17. The fixed network camera shall support Intelligent Defog to automatically adjust the contrast of the image in foggy scenes.
18. The fixed network camera shall offer comprehensive video content analysis capabilities, including detection and classification of persons and vehicles.
19. The fixed network camera shall offer a wide range of video analytics rule configuration, including:
a. Any object
b. Object in field
c. Line crossing
d. Enter / leave field
e. Loitering
f. Follow route
g. Idle object
h. Removed object
i. Counting
j. Occupancy
k. Crowd density estimation
l. Condition change
m. Similarity search
n. Flow / counter flow
o. Objects starting to move
p. Objects stopping
q. Tampering
r. Rule based alarms and tracking
s. Audio detection (May also be used to generate an alarm.)
20. The fixed network camera shall be configurable to execute the following actions upon alarm activation:
a. Turn its built-in output on or off
b. Turn another supported camera output on the same network on or off
c. Stream video to a compatible decoder
d. Send an e-mail with an image attachment
E Local SD storage
1. The fixed network camera shall have one microSD card slot that uses standard off-the-shelf SD (Secure Digital) up to 2 TB, SDHC (Standard Digital High Capacity) or SDXC (Secure Digital eXtended Capacity).
2. The fixed network camera shall support multiple recording modes, including manual, scheduled, pre-alarm and alarm recording.
3. The fixed network camera shall support health monitoring on the microSD card.
4. The fixed network camera shall support uploading JPEG images with video analytics overlay to an FTP server.
F Audio
1. The fixed network camera shall provide switchable audio input. This includes one (1) line-in level (10 kOhm typical, max. 1 Vrms) or one (1) microphone-in level (2.5 VDC, 4 mA). 
2. The fixed network camera shall provide one (1) audio line out (1.5 kOhm typical, 1 Vrms).
3. The fixed network camera shall provide two (2) alarm inputs and one (1) alarm output.
4. The fixed network camera shall offer the G.711 8 kHz, L16 16 kHz and AAC compression rates
5. The fixed network camera shall provide full duplex and half duplex streaming.
6. The fixed network camera shall be capable of disabling audio input permanently with a license code.
G ONVIF
1. The fixed network camera shall conform to the ONVIF Profile S, G, T and M.
H Video Analytics
1. The fixed network camera shall offer embedded deep learning-based detection and video analytics (IVA Pro) that eliminate dedicated PCs and associated software maintenance.
2. The fixed network camera shall offer embedded IVA Pro Buildings, IVA Pro Perimeter and IVA Pro Privacy for reliable deep learning-based detection.
3. The fixed network camera shall support other license options, including:
a. IVA Pro Traffic
b. IVA Pro Appearance
c. IVA Pro Visual Gun Detection
d. IVA Pro PPE
4. The fixed network camera shall provide Camera Trainer to allow the user to train the system for custom object detection and classification.
5. The fixed network camera shall be capable of running 16 different video analytics rules simultaneously.
6. The fixed network camera shall support automatic switching of video analytics types according to a predefined schedule.
7. The fixed network camera shall be capable of generating metadata, including object speed, geolocation, height, width, and classification to be recorded with the video.
8. The fixed network camera shall be capable of detecting and classifying up to 64 objects.
9. The fixed network camera shall support machine learning to enable users to classify customized objects.
2.04 NETWORK
A Connectivity:
1. The fixed network camera shall offer versatile network connectivity options, such as 10/100/1000BASE-T and Ethernet interfaces.
B Protocols supported:
1. The fixed network camera shall support the following protocols:
a. Transmission Control Protocol (TCP), Internet Protocol (IP) v4 and v6, User Datagram Protocol (UDP)
b. Configuration: Dynamic Host Configuration Protocol (DHCP) and fixed IP address
c. Web services: Internet Control Message Protocol (ICMP) and ICMP v6, Hypertext Transfer Protocol (HTTP), Secure Hypertext Transfer Protocol (HTTPS)
d. Network services: Address Resolution Protocol (ARP), Domain Name System (DNS), Network Time Protocol (NTP), File Transfer Protocol (FTP), System Network Management Protocol (SNMP) v3 and MIBII
e. Media: Real-Time Control Protocol (RTCP), Real-Time Transport Protocol (RTP), Real-Time Streaming Protocol (RTSP); Internet Group Messaging Protocol (IGMP), DiffServ (QoS)
f. Security: IEEE 802.1x Extensible Authentication Protocol (EAP)/Transport Layer Security (TLS)
C Data Security
1. The fixed network camera offers a built-in secure element with Trusted Platform Module (TPM) that supports RSA 4096 bit for device identity and AES/DES/PKI encryption.
2. The fixed network camera offers advanced handling certificates, including:
a. Pre-installation of manufacturer origin device certificate
b. Automatic generation of self-signed unique certificates when required
3. The fixed network camera supports full end-to-end encryption when used with supported VMS.
4. The fixed network camera supports different encryption protocols, such as TLS 1.2, AES 256, AES 128, and TLS 1.3.
5. The fixed network camera supports multiple video authentication methods, such as MD5, SHA-1, SHA-256, and Checksum verification.
6. The fixed network camera offers XTS-AES for local storage encryption.
7. The fixed network camera offers signed firmware, secure boot and software sealing functionalities to ensure firmware protection.
8. The fixed network camera shall be compliant with IEC62443-4-1 and UL 2900-2-3.
2.05 ELECTRICAL
A Power Input:
1. The fixed network camera shall support the following redundant power options:
a. 24 VAC
b. 12 to 26 VDC
c. PoE (IEEE 802.3at Type 1, Class 3)
B Power Consumption (maximum)
1. The fixed network camera shall support the following maximum power consumption options:
a. VAC: 14 W
b. VDC: 14 W
c. PoE: 12.95 W
2.06 MECHANICAL AND ENVIRONMENTAL
A Material:
1. The fixed network camera shall offer an anodized cast aluminum, rugged design and polycarbonate housing.
B Finish:
1. The fixed network camera shall offer a white and black finish.
C Dimensions (H x W x D):
1. The fixed network camera shall have 70mm x 80.2mm x 205 mm (2.76 in. x 3.15 in. x 8.07 in.)
D Temperature:
1. The fixed network camera shall support an operating temperature range of -20 °C to 55 °C (-4 °F to 131 °F).
2. The fixed network camera shall support a storage temperature range of -30 °C to 70 ºC (-22 °F to 158 ºF).
E Relative Humidity (non-condensing):
1. The fixed network camera shall support an operating relative humidity of 	5% to 93%.
2. The fixed network camera shall support a storage relative humidity of 0 to 100%.
F Ingress Protection
1. The fixed network camera shall offer IP5X environmental protection.
G Mounting:
1. The fixed network camera shall offer accessories to enable the mounting of the box camera in the following circumstances:
a. Wall/ceiling mount
b. Column mount
c. Pole mount
d. Corner mount
2.07 ACCESSORIES
1. UHO-HBGS-11		Outdoor housing, 24 VAC, feed-through
2. UHO-HBGS-51		Outdoor housing, blower, 230VAC/35W
3. UHO-HBGS-61		Outdoor housing, blower, 120VAC/35W
4. UHO-POE-10 		POE outdoor housing, heater, blower
5. VSP-UHO-POE-10	PoE outdoor housing IK10, heater, blower
6. LTC 9219/01		Feed through J mount
7. LTC 9210/01		Column mount, 8”, 9KG/20lb load
8. LTC 9213/01 		Pole mount adapter for LTC9210,9212,9215
9. LTC 9215/00		Wall mount with cable feed through, 12”
10. LTC 9215/00S		Wall mount for UHI/UHO
11. TC9210U		Camera mount, 6”, indoor
12. NBN-MCSMB-03M	Cable, SMB to BNC, camera-cable, 0.3m
13. NBN-MCSMB-30M	Cable, SMB to BNC, camera-monitor/DVR
14. NPD-5001-POE		Midspan, 15W, single port, AC in
15. NPD-5004-POE		Midspan, 4 portx 15W, AC in
16. MSD-064G		IP SECURITY MICROSD CARD 64G
17. MSD-128G		IP SECURITY MICROSD CARD 128G
18. MSD-256G		IP SECURITY MICROSD CARD 256G
19. NCA-WLAN-EU		Wireless installation dongle EU
20. NCA-WLAN-NA 	Wireless installation dongle NA
21. UPA-2450-50		PSU, 220VAC 50Hz, 24VAC 50VA out

END OF SECTION
PART  3    EXECUTION
3.01 INSTALLERS
A Contractor personnel shall comply with all applicable state and local licensing requirements.
3.02 PREPARATION
A The network design and configuration shall be verified for compatibility and performance with the camera(s). 
B Network configuration shall be tested and qualified by the Contractor prior to camera installation.
C Before permanent installation of the system, the Contractor shall test the system in conditions simulating the final installed environment.
3.03 INSTALLATION
A The contractor shall follow all Manufacturer-published guidance on proper installation and configuration of the installed cameras.
B The Contractor shall test the system in conditions simulating the final installed environment
C Reports:
1. System test results
2. System network addressing and device settings
3.04 STORAGE
A Products shall be stored in an environment where temperature and humidity are in the range specified by the Manufacturer.

END OF SECTION
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